**Spokane County Wildfire Debris**

Graham Road Waste Acceptance Requirements

***Construction & Demolition (C&D) Materials (“Wildfire Debris”)***

Required documentation:

* A conventional asbestos survey and/or alternate asbestos survey from an AHERA building inspector showing no asbestos
* An asbestos survey and certification from a certified asbestos abatement contractor that all ACM has been abated

Without the above documentation load will be rejected or must be managed as asbestos-containing waste material (ACM)

***Presumed Asbestos Debris***

All wildfire generated debris and ash may be considered presumed asbestos containing material (PACM) and managed following the requirements for ACM. Each load must arrive with approved documentation consisting of a completed Waste Shipment Record.

All loads of presumed or known ACM must follow the packaging requirements for acceptance of ACM. The requirements for packaging of these materials are as follows:

Adequately Wet

Generators are responsible to ensure that ACM is adequately wet as required by regulation prior to packaging.

6 mil bags (55gal Max)

All PACM and ACM must be double bagged in a 6 mil bag (55gal Maximum). Each bag must be sealed properly. Each bag must be labeled in compliance with the regulations.

* + Labeled bags are available at the scale house.
  + Labels must display the following information:

**ADDRESS (where the waste was generated)**

**NAME OF GENERATOR**

**DATE WASTE WAS COLLECTED (BAGGED)**

**DANGER**

**CONTAINS ASBESTOS FIBERS**

**MAY CAUSE CANCER**

**CAUSES DAMAGE TO LUNGS**

**DO NOT BREATHE DUST**

**AVOID CREATING DUST**

Burrito Wrapped Asbestos

Burrito wrapped asbestos must be double wrapped in **reinforced** 6 mil plastic.

Burrito style wrapped asbestos must have the seams glued and taped so they do not leak during transportation or offloading.

Burrito wrapped ACM must be marked in several locations as follows;

**ADDRESS (where the waste was generated)**

**NAME OF GENERATOR**

**DATE WASTE WAS COLLECTED (BAGGED)**

**DANGER**

**CONTAINS ASBESTOS FIBERS**

**MAY CAUSE CANCER**

**CAUSES DAMAGE TO LUNGS**

**DO NOT BREATHE DUST**

**AVOID CREATING DUST**

Any burrito wrapped loads arriving at the facility that are not double wrapped with re-enforced 6 mil plastic and properly labeled will be rejected.

Torn or Broken Packaging

When unloading, if at any time your packaging rips, tears or is breached in anyway it must immediately be repaired. All transporters shall carry plastic, tape and glue at all times so the repair can be completed.

Vermiculite Materials

Waste Management requires that all vermiculite be packaged and disposed the same as ACM as described above.

Graham Road Landfill reserves the right to prohibit any company that violates these policies from disposal of PACM or ACM at Graham Road LF. Any clean up or additional work required to dispose of improperly packaged or prepared ACM will be charged at the full rate allowable by law.

Dead animals, electronics, CFC containing appliances, and scrap metal are not acceptable at Graham Road Recycling and Disposal Facility.

|  |
| --- |
| GRAHAM ROAD RECYCLING & DISPOSAL FACILITY 1820 S. GRAHAM RD, MEDICAL LAKE, WA 99022 |
|  |
| **WASTE SHIPMENT RECORD** |  |
| **1. Work Site Name and Address** |  |
| Work Site Name: |  |
| Work Site Address: City: State/Zip: |  |
| Owners Name: |  |
| Mailing Address: City: State/Zip: |  |
| County: |  |
| Phone Number: |  |
| **2. Operator's Name and Address:** |  |
| Name: |  |
| Address |  |
| Phone Number: |  |
| **3. Disposal Site:** |  |
| Name: Graham Road Recycling and Disposal Facility |  |
| Site Mailing Address: 1820 S. Graham Rd, Medical Lake, WA 99022 |  |
| Phone Number: (509) 387-6279 |  |
| **4. Responsible Agency:** |  |
| Name: US EPA Region 10 WA DOE - EASTERN REGIONAL OFFICE |  |
| Address: 1200 6th Ave., Seattle, WA 98101 4601 N Monroe, Spokane, WA 99205-1295 |  |
| **5. Description of Materials:** |  |
|  |
| **6. Containers (quantity):** |  |
| **7. Total Quantity in Cubic Yards:** |  |
| **8. Special handling instructions and additional information:** ACM must be packaged correctly and adequately wet at the time of disposal. |  |
|  |
| **9. Operator's Certification:** I hereby certify that the above listed material(s) is(are) not hazardous as defined by 40 CFR Part 261, or applicable state law. I hereby declare that the contents of this consignment are full and accurately described above by proper shipping name, and are classified, packed, marked, labeled, and are in all respects in proper condition for transport by highway according to applicable international and government regulations. |  |
|  |
|  |
| **Printed Name: Title:** |  |
| **Signature:** |  |
| **10. Transporter 1 (Acknowledgement of receipt of materials)** |  |
| Printed Name: Title: |  |
| Address: |  |
| Phone Number: |  |
| Signature: |  |
| **11. Transporter 2 (Acknowledgement of receipt of materials)** *only complete if there is a change in Transporter 1* |  |
| Printed Name: Title: |  |
| Address: |  |
| Phone Number: |  |
| Signature: |  |
| **12. Discrepancy Indication Space:** |  |
| **13. Disposal Site Owner/Operator:** Certification of receipt of asbestos materials covered by this manifest except as noted in item 12. |  |
| Printed Name: Title: |  |
| Signature: Date: |  |